<div align=center>
<img src="https://github.com/BestModules-Libraries/img/blob/main/BMS36T001_V1.0.png" width="320" height="240"> 
</div> 


BMS36T001 
===========================================================

The Best Modules BMS36T001 is a shield board for IR proximity sensing with motor driver output function, which uses the UART communication method. This document provides the description of the BMS36T001 Arduino Lib functions and how to install the Arduino Lib. The example demonstrates the function of driving the motor forward when the module is in the sensing status and driving the motor to standby when the module is not in the sensing status.

This library can be installed via the Arduino Library manager. Search for **BMS36T001**. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **keywords.txt** - Keywords from this library that will be highlighted in the Arduino IDE. 
* **library.properties** - General library properties for the Arduino package manager. 

Documentation 
-------------------

* **[BMS36T001 Arduino Library V1.0.1 Description v100]( https://www.bestmodulescorp.com/bms36t001.html#tab-product2 )** - Arduino Library Description.

Version History  
-------------------

* **V1.0.1**  
&emsp;&emsp;- Initial public release.
* **V1.0.2**  
&emsp;&emsp;- Add function：getFWVer();  

License Information
-------------------

This product is _**open source**_! 

Please review the LICENSE.md file for license information. 

If you have any questions or concerns on licensing, please contact technical support on our BESTMODULES Email:service@bestmodulescorp.com

Distributed as-is; no warranty is given.

BESTMODULES
