Write BMZ00050 with RegisterMode:
                Write one page,Page0x40:0x40,0x40,0x40,0x40；
                Write two pages,Page0x41-42:0x41,0x41,0x41,0x41,0x42,0x42,0x42,0x42；

Read BMZ00050 with RegisterMode,print its data out to the Arduino Serial Monitor. 